Programming a USB Cherry keyboard with Designer.
·	Install the Cherry Tools Designer wither off the CD that came with the keyboard or from our setups CD in setups\drivers\cherry tools\fulledition\cherry_tools_english.msi
·	Plug in the keyboard and open the designer program from Start>All Programs>Cherry Tools>Designer
·	The program should automatically detect the keyboard and bring up an active configuration window.
·	On the left side you will see Track 1 and Track 2
·	Highlight Track 1.
            		Under Header check Enabled and click Edit. Type a % and click OK.
                 	Under Terminator check Enabled and click Edit. Type a ? and click OK.
    	Highlight Track 2.
             	Under Header check Enabled and click Edit. Type a ;(semi-colon) and click OK.
Under Terminator check Enabled and click Edit. Type a ? and hit Enter on the letterpad and click OK
·	Click on the Activate icon on the toolbar to program the keyboard with these settings.  You should get a windows that says The requested operation was completed successfully. Click OK.
·	It will bring up a window for you to test the magcard reader. Swipe a card and make sure the formatting is correct. Then you can exit the Designer.
 
Format : %Bcardnumber^Name^group of number?;cardnumber=Group of numbers?
	  And it should hit enter after the ? so the cursor is on the nest line.