Instructions for Programming Magtek 3 Track Reader

1.	Install MagTek Configuration software from Setups (Magtek Config.zip).

2.	Open MagTek USB software after install and wait for it to recognize the reader.

3.	After it recognizes it, click on the Send Commands

4.	To program the reader for two tracks enter 01 03 05 on the Send Message line and click Send Message.  You should see communication in the dialog box below.

5.	To save the programming, enter 02 and hit Send Message.  You will see dialog in the communication box again.  After that click on the Read Cards tab and swipe the card.  

To restore default settings use the command 01 03 95.  Then to save it, enter 02.